**Beat Extraction with Application to Robot Drumming**

~

Michael Engstrom

# Abstract

The goal of this project is to design a robot which can play drums in rhythm to an external audio source. The audio source can be either a pre-recorded track or a live sample from a microphone. The dominant beats-per-minute (BPM) of the audio would be extracted and the robot would drum in time to the BPM. A fast BPM extraction algorithm developed by Eric Scheirer was adopted and implemented. The main advantage of this algorithm is it has no prerequisite to decompose the audio information into notes beforehand and can therefore be automated.

The tasks of control of the robot motion and the BPM extraction of the input audio are separated. The main advantage of this approach is that by creating a generic interface between Input Logic and Robot Control each could be used independently for application to multiple robots or control systems. A host computer inputs audio from the environment (via microphone) and extracts the BPM data with the Scheirer algorithm to send to a robot controller. A commercially available robot controller was used to control the Drumming Robot servo motors and to interface with the host.

The Robot Theater at Portland State University features animated robots with the goal of performing music and acting out scenes for the entertainment of the audience passing through the halls of the FAB building. The Robot Drummer idea was conceived following the construction of a Handshaking Robot project involving the ‘DIM’ robot located in the PSU Robot Theater. By adding a second arm to the DIM torso and powering movement by servo motors and a robot controller, the motions of drumming could be performed for the Robot Theater. Audience members could play music, clap or otherwise make rhythmic noise and a microphone would input the audio to be processed to control the motion of the Drumming Robot.

Table of Contents

[Abstract ii](#_Toc447722056)

[List of Figures iv](#_Toc447722057)

[List of Equations v](#_Toc447722058)

[List of Tables v](#_Toc447722059)

[Chapter 1 – Introduction 1](#_Toc447722060)

[Beat Detection Audio Input 3](#_Toc447722061)

[BPM Algorithm Steps 4](#_Toc447722062)

[Step 1: Frequency Filterbank 4](#_Toc447722063)

[Step 2: Envelope Extractor 6](#_Toc447722064)

[Steps 3 and 4– Differentiate and Rectify Signal 11](#_Toc447722065)

[Step 5 – Comb Filter 12](#_Toc447722066)

[Chapter 2 – Host Side Software Design 15](#_Toc447722067)

[Algorithm Evaluation and Optimization 16](#_Toc447722068)

[Chapter 3 – Robot Design 20](#_Toc447722069)

[Robot Design – Software 20](#_Toc447722070)

[Robot Design – Servo Control 23](#_Toc447722071)

[Robot Design – Arms 25](#_Toc447722072)

[Chapter 4 – Testing and Implementation 28](#_Toc447722073)

[Chapter 5 - Conclusion and Future Work 30](#_Toc447722074)

[REFERENCES 32](#_Toc447722075)

[Appendices 33](#_Toc447722076)

[**A.** **Bill of Materials** 33](#_Toc447722077)

[**B.** **Robot Controller Code** 34](#_Toc447722078)

[**C.** **Host MATLAB Code** 52](#_Toc447722079)

# List of Figures

[Figure 1 – Beat Detection Diagram 2](#_Toc447722385)

[Figure 2 – Filterbank Bands 1, 3, 5 5](#_Toc447722386)

[Figure 3 – Filterbank Bands 2, 4, 6 5](#_Toc447722387)

[Figure 4 – Step 1: Frequency Filterbank 6](#_Toc447722388)

[Figure 5 – Hanning and Hamming Windowing Filters 7](#_Toc447722389)

[Figure 6 – Windowing Example in MATLAB 8](#_Toc447722390)

[Figure 7 - Signal Amplitude and Envelope 8](#_Toc447722391)

[Figure 8 – Signal Tempo vs. Energy 10](#_Toc447722392)

[Figure 9 – Step 2: Smoothing 10](#_Toc447722393)

[Figure 10 – Half-Wave Rectification 11](#_Toc447722394)

[Figure 11 – Step 3: Differentiation and Step 4: Rectification 12](#_Toc447722395)

[Figure 12 – Step 5: Comb Filter 12](#_Toc447722396)

[Figure 13 – Parameter Optimization Results 18](#_Toc447722397)

[Figure 14 – Atmel Studio 20](#_Toc447722398)

[Figure 15 – Robot Controller State Machine 21](#_Toc447722399)

[Figure 16 – Robot Controller and Servo Motor 23](#_Toc447722400)

[Figure 17 – Servo Pulse Waveform 24](#_Toc447722401)

[Figure 18 – Robot Elbow Range of Motion 26](#_Toc447722402)

[Figure 19 – Robot Shoulder Left/Right Motion 26](#_Toc447722403)

[Figure 20 – Robot Shoulder Up/Down Motion 27](#_Toc447722404)

[Figure 21 – Robot Arm Mounted on Robot Torso 27](#_Toc447722405)

# List of Equations

[Equation 1 – Hanning Windowing Filter 7](#_Toc447722889)

[Equation 2 – Fourier Transform 9](#_Toc447722890)

[Equation 3 – Discrete Fourier Transform 9](#_Toc447722891)

[Equation 4 – FIR Filter Response 11](#_Toc447722892)

[Equation 5 – Magnitude Response 13](#_Toc447722893)

[Equation 6 – Local Maxima Unity 13](#_Toc447722894)

[Equation 7 – Output Signal 13](#_Toc447722895)

[Equation 8 – BPM Granularity 16](#_Toc447722896)

[Equation 9 – Calculated Error 17](#_Toc447722897)

# List of Tables

[Table 1 – BPM Granularity for Parameter Testing 17](#_Toc447726885)

[Table 2 – Algorithm Parameter Set 17](#_Toc447726886)

[Table 3 – Optimized Parameter Set 18](#_Toc447726887)

[Table 4 – Parameter Set: No Scaling 19](#_Toc447726888)

[Table 5 – Loop Delay Calculation 22](#_Toc447726889)

[Table 6 – Orangutan Robot Controller Specifications 24](#_Toc447726890)

[Table 7 – Bill of Materials 33](#_Toc447726891)

# Chapter 1 – Introduction

Music is composed of multiple acoustic elements which combine to be interpreted as tempo, melody, beat, etc. The human ear is very adept at psychoacoustic discernment of these elements in the music as a whole. Tempo includes counterpoint, grouping, and hierarchy which are subtly combined and interpreted by the human ear. In electronic decomposition of music or other repetitive audio, it is apparent that tempo is complex while the beat or pulse (BPM) is simple. [Handel, 1989] Handel continues that beat in music is the ‘sense of equally spaced temporal units’ and as a repeating pattern is a candidate for frequency derived mathematical decomposition such as Fourier Transforms.

Fourier Transforms can detect frequency power trends to determine the beat of an audio sample. This decomposed audio beat information can be used to control mechanical output, such as the Drumming Robot. In his paper ‘Tempo and beat analysis of acoustical musical signals’ Eric Scheirer describes a beat extraction algorithm which is effective in determining the BPM of an audio sample [Scheirer, 1996]. The use of Fourier Transforms is effective for immediate analysis of BPM information.

In the Drumming Robot project, the Beat Extraction algorithm is implemented and explored for use in controlling the Drumming Robot. The program variables were parameterized using a range of inputs to evaluate the algorithm, with description and results shown later in this paper. By testing multiple parameter combinations it was possible to optimize the accuracy and speed of the algorithm while the performance for the audience was improved.

A host Input Logic system which sends BPM data over a communication port does not need to know the configuration of the robot which implements the drumming motion. A drumming robot listening to a communication port for BPM audio control information does not care how the BPM information is obtained. It only cares about the data and is responsible for implementing the resulting BPM motion. The design and test of such a Logic-Control system is thereby simplified. The Input Logic system only needs to be accurate as far as beat extraction and BPM output.

Any robot could use the BPM information for a variety of unknown tasks beyond drumming. The Robot Control system only needs to be able to input the BPM data and accurately implement the drumming. Any input, as long as it is in the correct format, can be used with this drumming robot. This includes other BPM extraction methods approaching real-time input.

A drumming robot is preferred to have human-like motion. It has been observed that articulating lamp sections resemble jointed limbs. This fact has been leveraged for this project. Two lamps were dismantled so that the remaining portion hinged like an elbow, and swivel connectors were added to the top of the robot arm to simulate shoulder rotation and swing. This construction resulted in three degrees of freedom for each arm, or six degrees of freedom total.

This flow diagram is followed by an explanation of the algorithm steps:



Figure – Beat Detection Diagram

* Beat Detection Algorithm steps:
  1. Frequency Filter Bank
     + Split frequency range of sample into smaller segments
  2. Envelope Extraction (Fourier Transform)
     + Frequency power is extracted
  3. Differentiation
     + Smoothing of extracted signal
  4. Rectification
     + Isolation of desired frequency information
  5. Multiple Comb Filters (Resonant Filterbank)
     + Match frequency sample to known BPM
     + Peak-Picking
     + Best Fit is our desired BPM output

## Beat Detection Audio Input

The host-side processing of audio for BPM detection begins with a choice of inputs: microphone samples or stored .wav files. MATLAB offers the benefits of built-in sound device input, matrix manipulation for audio data, Fourier processing functions, and serial connection functions. The host is entirely responsible for the algorithm which extracts the BPM from audio input, then that information is sent over a serial connection to the robot controller. This project uses MATLAB entirely for performing these host-side operations.

For live sound input a microphone is sampled and the digital data stored with as a 8000 Hz, 8-bit, single channel array in MATLAB. Stored .wav files (for example, music or click tracks) are digitized using the center of the file. Resulting data arrays both have a sample frequency that can be varied as a parameter from 2048 to 16384 in powers of 2. This affects the accuracy as well as the processing time of the algorithm.

## 

## BPM Algorithm Steps

### Step 1: Frequency Filterbank

The input audio sample is split into several frequency ranges, and each range is passed through the BPM algorithm. This is targeted for audio samples such as music, which varies in frequency range according to the variety of instruments used. Different instruments use different frequency bands, and a frequency Filterbank allows for different instruments to be detected. Most rhythm instruments use the lower frequency spectrum (0-200 Hz). Some audio samples exhibit only a small frequency range. An example of this is ‘click tracks’ (audio files created to have a specific BPM by repeating a pulse signal for the duration of the file). For this algorithm the Filterbank split is:

0-200Hz, 200-400Hz, 400-800Hz, 800-1600Hz, 1600-3200Hz

Each filter is implemented using a sixth-order elliptical filter. This results in 3dB of ripple in the passband and 40 dB of rejection in the stopband, with sharply defined ranges for each frequency band. Most BPM information for audio tracks is located in the 0-200Hz band (correlating with rhythm instruments such as drums and bass). Melody, vocal and harmony elements in music tends to be located in the higher band frequencies but are also less likely to follow the beat as closely. [reference?] Below is a plot of the bands, separated to show the drop-offs:



Figure – Filterbank Bands 1, 3, 5



Figure – Filterbank Bands 2, 4, 6



Figure – Step 1: Frequency Filterbank

### 

### Step 2: Envelope Extractor

Next an Envelope Extractor is used to filter each of the signal segments. The audio sample segments are converted from the Time Domain to the Frequency Domain using a Fast Fourier Transform (FFT) derived formula. Since the samples are already in digital form, a Discrete Fourier Transform (DFT) is used. The Fourier Transform separates the frequency and magnitude components of the signal. In the Time Domain the signal would be convolved to extract the data, but this is complex to perform. Converting the sample to the Frequency Domain and multiplying is the same operation but much simpler to perform (and faster, which is always a consideration for real-time signal processing calculations)

The signal is then transformed using a Hanning Window to clean up the frequency range and improve signal clarity [National Instruments]:



Equation – Hanning Windowing Filter

Windowing the input signal can improve the accuracy of the resulting signal. Two of the most popular windowing functions are Hamming and Hanning (Hann) windows. The main difference is how sharply the resulting signal is when multiplied by the input signal. Hamming windows offer a sharper center frequency but the Hanning window reduces the side lobe amplitude away from the center frequency. For this project it is desired to lower the non-center frequency amplitude to improve the result of later multiplying the signal with the comb filters. Therefore the Hanning window is a better choice [source = NI]:



Figure – Hanning and Hamming Windowing Filters

Windowing also limits the inclusion of partial-period waves which can skew the FFT, also known as ‘spectral leakage’. With windowing the signal is zero outside a chosen interval which improves the result in the desired range. Using the MATLAB Window Visualization Tool, the effects of windowing on a signal can be observed. This is shown with an example of a generated signal using N = 64:




Figure – Windowing Example in MATLAB

Below is an example of an input signal before windowing (left) and after (right). Notice that the data shape is retained but duplicated signal information is removed and noise is reduced:



Figure - Signal Amplitude and Envelope

Signal processing is greatly simplified by performing these complex Time Domain operations in the Frequency Domain using the Fourier Transform. The transformed signal is then converted back to Time Domain using an inverse Fourier Transform. Converting a signal from the Time Domain to the Frequency Domain is performed mathematically with the Fourier Transform Pair where *X(f)* is the Frequency Domain signal and *x(t)* is the Time Domain signal:



Equation – Fourier Transform

It is assumed that the input signal *x(t)* is periodic when considered from negative infinity to positive infinity. For this digital audio sampling project our sound sample is not infinite but finite. Since the sample is already stored as discrete data points it is desired to use the Discrete Fourier Transform for digital signals, which in this form:



Equation – Discrete Fourier Transform

After the original signal is converted to the Frequency Domain by using the Fourier Transform the data is represented in a frequency spectrum as a measure of power. The BPM Algorithm assumes that the beat frequency of a music sample will correspond with FFT frequencies that have the most power. Later, comb filters with known frequencies will be used to determine the best BPM candidate. Below is an example of an FFT of an input signal, showing highest frequency power at about 150 BPM and a slightly less power peak at 75 BPM.




Figure – Signal Tempo vs. Energy

This harmonic effect can be expected at multiples of BPM values for given audio input samples. For this project the BPM range is limited from 60-120 BPM, so the example below would be considered to be 75 BPM even though it has slightly less power than the harmonic at 150 BPM.




Figure – Step 2: Smoothing

In algorithm steps 3 and 4 the signal is further processed to improve the accuracy of the final BPM determination.

### Steps 3 and 4– Differentiate and Rectify Signal

The differential of each digital sample to the next is calculated and retained only in case of positive results, giving a half-wave rectified output signal. Differentiating a signal in MATLAB is accomplished with the diff function, which is seen as a first order finite impulse response (FIR) filter with a response of



Equation – FIR Filter Response

The input signal is processed with a half-wave rectify step. This helps accentuate the sound changes in the signal, which corresponds to beats. Rectifying a signal is trivial in MATLAB. For half-wave processing the positive wave portion is kept and the negative wave set to zero. In MATLAB the difference from one sample to the next of the input signal is derived. The result is retained only if the difference is positive, and the signal is now half-wave rectified. Below is the input sine wave (red) and half-wave output (blue):



Figure – Half-Wave Rectification

*(Source: Analog Devices WiKi page)*

Next is a MATLAB example of the input signal which has been differentiated and then half-wave rectified.



Figure – Step 3: Differentiation and Step 4: Rectification

The higher power peaks are isolated and allow for better accuracy when using comb filters in the next step. The comb filter step gives a determination of the best-fit BPM of the input signal.

### Step 5 – Comb Filter



Figure – Step 5: Comb Filter

The final algorithm step determines the best estimate of BPM for an input signal. Convolution of the signal in the Time Domain with successive comb filters of increasing, known BPM values results in power products of the signal and comb filters. The best fit BPM is simply the product that has the highest power product. Derivation of convolution is complex in the Time Domain, which is why the signal is converted to the Frequency Domain using the FFT, changing the convolution operation to a simple multiplication operation. In Step 2 the Beat Detection Algorithm the Fourier Transform of the signal was derived, resulting in a power spike at one or more frequencies, according to the frequency energy. This is multiplied by comb filters of increasing BPM.

A Comb Filter is used to find tempo maxima. For delay *T* and gain *α* the magnitude response is




Equation – Magnitude Response

Local maxima are wherever is near 1 at the *T*th roots of unity, expressed as



Equation – Local Maxima Unity

If we stimulate a comb filter with delay *T* and gain *α* with a right-sided pulse train of height *A* and period *k* we get reinforcement (resonance) if *T*=*k*. Let and be the input and output signals at time *t*, then



Equation – Output Signal

For our purposes, if a comb filter energy response is higher than a previous ‘best fit’ comb filter(when compared to the input sample) we discard the previous result and keep the new comb filter as our ‘best fit’. This final value is our BPM determination and the Beat Detection Algorithm is complete. Next is a discussion of implementing the algorithm in software.


# Chapter 2 – Host Side Software Design

The Scheier BPM Algorithm was implemented on the host using MATLAB scripts. A group from MIT developed a related project to detect the BPM from input files, and the code for this project uses core functions to perform the BPM evaluation. [reference] MATLAB was chosen for the built in functions for accessing audio input using computer microphones, a core goal of this project for use in the PSU Robot Theater. MATLAB also has functions for establishing serial communication links, as mentioned in chapter 2.

In the project planning stages the decision was made to develop the host BPM extraction feature separately from the Robot Controller development. This decision was made in part because the host and controller use different technologies (MATLAB and C code Atmel/Orangutan Robot Controller, respectively). The major benefit, however, of separating the host and controller by a serial connection is that each can be used in a modular ‘black box’ scenario. The Robot Controller is agnostic to the method used to extract the BPM information from an audio source and only listens to the coded control byte information provided by the serial input. Similarly, the host sends the BPM control information over the serial output to the Robot Controller but the control bytes could be used by any end device which is connected. This allows for the Robot Theater to control the BPM of the Drumming Robot with any BPM extraction method or desired control.

The Beat Extraction Algorithm steps are implemented in several corresponding MATLAB files, with a main script calling the others. This is all wrapped in a user input script that establishes a serial connection and determines whether the audio source is from a file or the input will be from the system microphone. In the microphone input mode the microphone audio input is processed for BPM information, the control byte sent over the serial connection, and then loops back to repeat these two steps until the user exits the MATLAB script. In this way the Robot Controller is continually receiving the most current BPM information available to the microphone. The byte value of a-z which is sent to the Robot Controller over the serial connection corresponds to the output of the BPM algorithm.

The MATLAB code describes the user interface for calling the Scheirer BPM Algorithm functions and calls the BPM functions in MATLAB with the audio data stored in a matrix. This audio data is passed from function to function in the BPM algorithm until the output result is an integer value from 60-120. The wrapper code then sends a control byte of a-z over the serial connection, to be handled by the Robot Controller (see Chapter 4). Since the BPM range of the project is 60-120 inclusive (61 BPM values) and there are 25 control bytes (a-y, z is only used as a PAUSE command) the granularity of BPM accuracy is calculated as



Equation – BPM Granularity

Below is pseudo code for implementing the Beat Detection Algorithm in MATLAB:

* Implementing in MatLAB
  + Input audio from file or microphone
    - .wav file or 10 seconds of microphone sample
  + Follow Handel Algorithm in Matlab
    - Result is BPM value
  + Send BPM control value using Serial connection to Robot Controller
    - Serial interface between host and controller
    - Change speed and tempo of robot drumming arms according to inputs

A full printout of the code is attached at the end of the project. Since the MATLAB BPM algorithm is spread over multiple files, the following flowchart helps explain the data flow and algorithm steps. The input file to the algorithm is the digital audio matrix:

## Algorithm Evaluation and Optimization

Once the software was working it was important to optimize the function. The performance of the beat extraction algorithm varies with the given parameter set. Two goals were determined to be essential for this project: BPM accuracy, as determined by percent error deviation from a known BPM; and time, as determined from when an audio sample was entered and the resultant BPM value. This project uses MATLAB to input the audio, calculate the BPM value, and send the data over a serial connection to the Orangutan robot controller. A set of ‘click tracks’ were created using Audacity with known BPM values. The range of 60-120 BPM was included, in 5 BPM granularity, and a few outlier BPMs were added to test robustness. The set includes:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Beat: | 35 BPM | 55 BPM | 60 BPM | 65 BPM | 70 BPM | 75 BPM | 80 BPM | 85 BPM |
| 90 BPM | 95 BPM | 100 BPM | 105 BPM | 110 BPM | 115 BPM | 120 BPM | 125 BPM | 145 BPM |


Table – BPM Granularity for Parameter Testing

For each set, parameters were varied and the resultant time per BPM and averaged error from the known BPM were measured and graphed. Parameters used:

|  |  |
| --- | --- |
|  | Range |
| Band Limits | None to [0 200 400 800 1600 3200] |
| Sample Rate | [2048, 4096, 8192, 16384] |
| Scaling | [0.75, 1.0, 1.25, 1.5] |

Table – Algorithm Parameter Set

This experiment resulted in 20 different Time vs. Error data points. These were graphed for comparison. The goal for calculation time was to be under 10 seconds, and for error it was less than 10%.



Equation – Calculated Error

Figure – Parameter Optimization Results

Looking at the graph, the data point with 4.5 seconds calculation time and 4.51% average error for the BPM came in at less than half our maximum goals. This data point corresponds to:

|  |  |
| --- | --- |
| (4.5s, 4.51%) | Range |
| Band Limits | None to [0 200 400 800 1600 3200] |
| Sample Rate | [2048, 4096, 8192, 16384] |
| Scaling | [0.75, 1.0, 1.25, 1.5] |

Table – Optimized Parameter Set

Using this as the final parameter set, we can be confident that our input algorithm is relatively fast and accurate. It also eliminates a major feature of the Handel algorithm, the splitting up of the band into smaller band limits. The parameter set that meets our time and error goals, while using the band limits and no scaling is the data point with 6.6 seconds calculation time and 8.25% average error for the BPM:

|  |  |
| --- | --- |
| (6.6s, 6.18%) | Range |
| Band Limits | None to [0 200 400 800 1600 3200] |
| Sample Rate | [2048, 4096, 8192, 16384] |
| Scaling | [0.75, 1.0, 1.25, 1.5] |

Table – Parameter Set: No Scaling

The time and error for the (6.6s, 6.18%) parameter set are acceptable. However, for the operation of the robot speed and accuracy are desired so the parameter configuration used will be the (4.5s, 4.51%) shown above.

# Chapter 3 – Robot Design



Figure – Atmel Studio

## Robot Design – Software

The Orangutan Robot Controller is designed to be compatible with Atmel Studio Development Software, a free development program available for download via links from the Pololu website. After installing the program and starting a new project the desired target device is chosen (Orangutan with the ATMega1284P processor in this case) and a C programming environment is opened. Many sample projects are available for controlling the features of the Orangutan robot controller, as well as the rich API features available in the project libraries. For this project the Servo, LED, LCD and Serial sample projects were extremely useful as code references.

For the robot controller side of this project a looping program initializes the servos, serial interface, and LCD display, then sets the arms to drum in 60 BPM. Button inputs allow for increase or decrease of BPM. In addition, the Orangutan continually listens for serial byte inputs of [a,z] (corresponding to BPM granularity of 2 BPM increments of 60-120). A state machine controls which BPM the robot is drumming to. Buttons can only increment sequentially from 60 to 120, but a detected serial input will immediately put the Drumming Robot in the desired BPM mode. Below is a state machine diagram showing the button and serial inputs, as well as the BPM delay and LCD output.



Figure – Robot Controller State Machine

The robot controller program is designed to capture user input for setting the state machine. This design is implemented in a similar framework as many other microcontrollers targeting real-time operation, and runs in a loop:

* Check serial input
  + If serial byte input of ‘a’-‘z’ detected
    - Set state
    - Use LCD to notify user of serial character detected
* Check button input
  + If Button1, increment state
  + Else if Button3, decrement state
    - Set state
* Perform delay for current BPM state
* Output LCD and LED information regarding BPM and mode

The serial communication is bidirectional. Pressing the middle button on the Orangutan sends a string message of “Robots Rule” back to the host. A simple feedback operation of sending a copy of each received control byte allows the host to verify that the Orangutan has the correct byte. It is also possible to send other information such as servo position, servo speed, loop delay and other pertinent values. This is not currently implemented. Below is a table showing the input bytes, Robot Controller states and the necessary delay needed per loop for the desired BPM cadence:

|  |  |  |  |
| --- | --- | --- | --- |
| **Input** | **Mode** | **BPM** | **Delay(ms)** |
| a | 1 | 60 | 500 |
| b | 2 | 62 | 484 |
| c | 3 | 65 | 462 |
| d | 4 | 68 | 441 |
| e | 5 | 70 | 429 |
| f | 6 | 72 | 417 |
| g | 7 | 75 | 400 |
| h | 8 | 78 | 385 |
| i | 9 | 80 | 375 |
| j | 10 | 82 | 366 |
| k | 11 | 85 | 353 |
| l | 12 | 88 | 341 |
| m | 13 | 90 | 333 |
| n | 14 | 92 | 326 |
| o | 15 | 95 | 316 |
| p | 16 | 98 | 306 |
| q | 17 | 100 | 300 |
| r | 18 | 102 | 294 |
| s | 19 | 105 | 286 |
| t | 20 | 108 | 278 |
| u | 21 | 110 | 273 |
| v | 22 | 112 | 268 |
| w | 23 | 115 | 261 |
| x | 24 | 118 | 254 |
| y | 25 | 120 | 250 |

Table – Loop Delay Calculation

## Robot Design – Servo Control

In examining jointed robots it was observed that many of these robots used servo motors (servos) directly as the joints. However, servos can be damaged by excessive torque and need to be programmed to limit motion which does not mimic human motion. One of the advantages of using lamp arms is the range of motion is very human-like, and the joint motion functions whether servos are working or not. In this project, servo motors were attached externally to the arms and linkages and springs were used to provide the powered range of motion. This mimics human arms with ‘muscles’ (servos) and ‘tendons’ or ‘ligaments’ (springs or brackets).

Servos are an inexpensive method of implementing motion for robots. For this reason, control boards were researched for features that would allow for effective servo control. Several types of control boards with HDL programming requirements were researched, and the Orangutan Robot Controller Board from Pololu was chosen for this project. The Orangutan is relatively cheap yet it can control 8 servos using C++ API interface calls, as well as 8 more using general-purpose IO ports and lower level programming.



Figure – Robot Controller and Servo Motor

The Orangutan boards can be purchased at www.pololu.com for about $100, and downloads are available with many examples for the boards. Someone with no previous knowledge of robot controllers (but with some C++ programming experience) can quickly implement, compile and flash example designs to the Orangutan board and experiment with modifying the behavior.



Table – Orangutan Robot Controller Specifications

Servos are fairly simple to use, just give them 3.3V to 6V and a control signal and the arm moves to a position. Most have a range of movement of 180°, with the control signal square-wave pulse running at 50 Hz and 1-2 ms ‘high’ time. Changing the pulse signal changes the arm position. 1ms is one extreme, 2ms is the other, and 1.5 ms pulses put the arm about in the middle. The APIs available in the Atmel-Programmed Orangutan controller easily control the position and speed of servo movement.



Figure – Servo Pulse Waveform

The Orangutan SVP 1284 board has eight onboard hardware servo controllers, two motor controllers, three serial interfaces (on USB and two UART) and button inputs. Outputs include LEDs and an attached backlit 2x14 character LCD, as well as multiple programmable IOs. The Orangutan can be powered and programmed via USB, but for servo use a battery pack power supply was necessary. Later this was replaced with a AC power supply which provided enough power to run the board and attached servos.

An issue with servos is the current reflection in response to a control signal. When the signal is sent and the servo motor responds with movement, it also generates a reflected current to the control board. This can interfere with the operation of the control board in the form of power loss, restarts and even corruption of the programmed flash image. The Orangutan can run low-power operations such as the LCD display, LEDs and beeping noises with just the USB attached (although the cable can get alarmingly hot). However, servos require more power to operate and have the current reflection issue as mentioned. Auxiliary power via battery pack (for mobile use) or power supply (stationary use) worked well for the six servos used in this project.

## Robot Design – Arms

The Drumming Robot Arms needed an attachment point for operation, and the DIM robot (as seen in the Robot Theater window) was chosen since it had no arms and was in proportion to a human in stature. Part of the goal for the project was to simulate human movement and form wherever possible. Therefore, in addition to lamp arms for the drumming arms they were attached to the DIM torso so as to mimic human shoulders using caster wheels (minus the actual wheels). Hobby plates and bolts were attached with nested servos to provide the torque for 1 DOF (Degree of Freedom) lower arm/elbow and 2 DOF shoulder movement.

One of the goals of the robot arm design was to mimic human drumming motion. The lamp arm was a good choice since it was already designed to be limited to a 180° range and resembled the range of the human elbow. There was a functional advantage in avoiding servos for arm joint attachment. If a servo failed, it could easily be replaced without disassembling the joint. Hobby straps were used to extend the swing of the servo motion and thus reduce the amount of torque applied directly to the arm servo. Event with high-torque metal gear servos (as used in this project) the load weight of the lower arm was high. Springs, reused from the original lamp arm, were used to counter this arm weight.




Figure – Robot Elbow Range of Motion

The shoulders were more interesting. The initial design included a simple hinge to attach the arms with 1 DOF. While searching for parts to construct the drumming robot it was noted that a caster wheel is a 2 DOF object. Using a sufficiently large caster wheel frame it was possible to fit a pair of servo motors into the frame with the wheel removed (actual wheel not needed). The axle holes were drilled out to fit the arm post for left-right arm motion. As seen in the picture a combination of hobby brackets, bolts, and a servo accomplishes this motion. Using another hobby bracket, heavy wire, and a servo enables up-down shoulder rotation to lift the arm up and down.



Figure – Robot Shoulder Left/Right Motion



Figure – Robot Shoulder Up/Down Motion



Figure – Robot Arm Mounted on Robot Torso

# Chapter 4 – Testing and Implementation

The robot arms were attached to the torso and the servos connected to the Orangutan robot controller for initial testing. This was initially performed using the controller-side software and buttons. The host and controller were designed separately and could be tested separately. The plan for testing the controller was first to use the on-board buttons to control the BPM states, second to send control bytes over the serial connection using a tty terminal (such as PuTTY), then third to send control bytes using the host BPM software.

The servos were required to be calibrated. The arms’ attached drumsticks were not striking the drum head in a precise position, causing skips in beats when too high and stressing the servo motors when too low. These values were changed in the robot controller software until the up and down distance was correct. This corresponds to changing the interval between servo control pulses, as described in ‘Orangutans and Servo Control’ previously.

After increasing the BPM values it was also observed that at higher BPMs the arms were no longer striking the drum head. The drumsticks did not have enough time at higher BPMs to strike the head before the loop ended and the servos began to move to the up position. This was corrected by increasing the servo speed value so at higher BPM loops the servos moved faster to their up or down position. As described in the ‘Orangutans and Servo Control’ section this is achieved by increasing the width of the servo control pulses. The arms were now accurately striking the drums with the drumsticks through the target 60-120 BPM range.

The calculated loop delay values were tested (counted over the space of a minute) for BPM accuracy and found to be correct. However, since each arm moved in the loop, the perceived BPM was twice the desired value. Also, the sound of the drumsticks quickly became monotonous after hours of testing. Both of these issues were addressed by making a single change to the robot control software: the left arm randomly chooses up or down servo arm positions each loop while the right arm continues to steadily alternate between up and down. This allows the right arm to always strike the correct BPM, while the left arm gives a random accompaniment to the performance of the Drumming Robot. The resulting rhythm is varied and changing, yet stays with the target BPM.

Next, host control was added to the test scenario. A serial connection was established with the drumming robot and known control byte values were tested through the BPM state machine states. The response time was under 0.5 seconds from keyboard strike to state change. Next, the host BPM algorithm software was successfully used to input sound from a microphone and send the BPM control byte over the serial connection to the robot controller. Finally the host software was modified to run in a loop so that it is continually capturing audio, extracting the BPM using the Scheirer Algorithm, and sending the control byte to the robot controller. The Robot Drummer was complete!

# Chapter 5 - Conclusion and Future Work

This has been a satisfying project. The goal of a functional Drumming Robot system has been accomplished. On the host side the laptop microphone inputs external audio, and accurate BPM information is extracted using MATLAB and the Scheirer Algorithm. This information is sent to the controller, which performs a percussive drumming pattern using servo-powered robot arms and a drum head. By separating the development of extraction and execution the project is useful for various timekeeping robots (not just drumming) as well as any project requiring BPM information in real time.

A strong framework of matrix manipulation, Fourier function support and hardware interfacing made MATLAB a good medium for implementing the Scheirer BPM Algorithm. By parameterizing the inputs to the BPM functions it was possible to perform multiple variations of bandwidth and precision. After examining these results it was observed that one of the core aspects of the Scheirer Algorithm, filterbanks, aligned with the poorest performing parameter sets. Omitting filterbanks also greatly reduced the computation time. This in turn allowed the use of higher audio sample rates, improving the overall accuracy of the BPM results and a better user experience. The error percentage is less than 5% while the speed is less than 5 seconds.

The Orangutan robot controller was a good choice for implementing the movement and logic of the Drumming Robot. The Orangutan used an Atmel Studio C language development environment with a rich library of API functions to control the servo motors, buttons, LEDs and other features available with the robot controller. It is useful as a standalone manually controlled device, but also allows remote BPM input and control from the host over the serial connection. An audience can control the Drumming Robot using the buttons for a specific BPM, or the system can run in a continual loop where microphone audio BPM data is extracted and controlling the Drumming Robot BPM.

Currently the Drumming Robot has six degrees of freedom between the shoulder and elbow control. In future work, the robot could be improved by adding more limbs (legs or more arms) and varying the percussion instruments. A bass drum, cowbell, floor tom or cymbal would give the audience a better experience. Also, the Scheirer BPM Algorithm could be implemented on the robot controller. However, there is no guarantee that this would be an improvement in speed. It is possible and even likely that a host-based processor and memory greatly outweigh the performance of the Orangutan. Also, the audio extraction is a problem on the Orangutan since it has no onboard microphone. Maybe a future solution would be to use a different controller with the inputs and processing capabilities to input audio and perform Fourier operations in a reasonable amount of time.

# REFERENCES

* *Tempo and beat analysis of acoustic musical signals*
  + Scheirer, Eric D.
  + MIT Media Laboratory, 1997
* Beat Sync Project
  + <http://www.clear.rice.edu/elec301/Projects01/beat_sync/>
  + Rice University, 2001
* *Listening*
  + Handel, S.
  + MIT, Cambridge, MA, 1989
* A Systolic FFT Architecture for Real Time FPGA Systems
  + Preston A. Jackson, Cy P. Chan, Jonathan E. Scalera, Charles M. Rader, and M. Michael Vai
  + MIT Lincoln Laboratory, 2004
* VLSI Report
  + Vincent Buso
  + Illinois Institute of Technology, 2012
* Hardware Implementations of the Fast Fourier Transform (FFT)
  + Sabih H. Gerez
  + University of Twente, The Netherlands, 2013
* Digital Signal Processing with Field Programmable Gate Arrays
  + U. Meyer-Baese
  + 3rd edition, Springer, 2007

# Appendices

1. **Bill of Materials**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item Image** | **Description** | **Cost** | **Quantity** | **Subtotal** |
| |  | | --- | |  | | Metal Straps - Pack of 20 | $ 12.98 | 1 | $ 12.98 |
| |  | | --- | |  | | 5" Rubber Swivel Caster | $ 22.96 | 2 | $ 45.92 |
| |  | | --- | |  | | Machine Screws + Nuts Kit | $ 3.97 | 1 | $ 3.97 |
| |  | | --- | |  | | Tower Pro MG995 High Torque Metal Gear Servo | $ 9.99 | 6 | $ 59.94 |
| |  | | --- | | OrangutanSVP.jpg | | Orangutan SVP-1284 Robot Controller from Pololu | $ 99.95 | 1 | $ 99.95 |
| |  | | --- | |  | | Swing Arm Lamp | $ 10.00 | 2 | $ 20.00 |
|  |  |  | **Total** | $ **242.76** |

Table – Bill of Materials

1. **Robot Controller Code**

#cs/\* ECE\_MastersThesis\_DrummingRobot - an application for the Pololu Orangutan SVP

\*

\* This application uses the Pololu AVR C/C++ Library. For help, see:

\* -User's guide: http://www.pololu.com/docs/0J20

\* -Command reference: http://www.pololu.com/docs/0J18

\* -Author: Michael Engstrom

\*

\*/

#ce

#include <pololu/orangutan.h>

#include <string.h>

#cs /\*

\* To use the SERVOs, you must connect the correct AVR I/O pins to their corresponding

\* servo demultiplexer output-selection pins on the Orangutan Robot Controller.

\* - Connect PB3 to SA.

\* - Connect PB4 to SB.

\*/

#ce

; This array specifies the correspondence between I/O pins and DEMUX

; output-selection pins. This demo uses three pins, which allows you

; to control up to 8 servos. You can also use two, one, or zero pins

; to control fewer servos.

;const unsigned char demuxPins[] = {IO\_B3, IO\_B4, IO\_C0}; ; select for eight servos

const unsigned char demuxPins[] = {IO\_B3, IO\_B4}; ; select for four servos

;const unsigned char demuxPins[] = {IO\_B3}; ; select for two servos

;const unsigned char demuxPins[] = {}; ; select for one servo

static unsigned char init\_speed = 150;

static unsigned int neutral\_servo\_pos = 1300;

static unsigned int rt\_shoulder\_rot\_lt = 2000;

static unsigned int rt\_shoulder\_rot\_rt = 1600;

static unsigned int rt\_shoulder\_rot = 1600;

static unsigned int rt\_elbow\_up = 1950;

static unsigned int rt\_elbow\_dn = 1550;

static unsigned int rt\_elbow = 1800;

static unsigned int lt\_shoulder\_rot\_lt = 1200;

static unsigned int lt\_shoulder\_rot\_rt = 850;

static unsigned int lt\_shoulder\_rot = 1200;

static unsigned int lt\_elbow\_up = 2050;

static unsigned int lt\_elbow\_dn = 2400;

static unsigned int lt\_elbow = 2200;

; receive\_buffer: A ring buffer that we will use to receive bytes on USB\_COMM.

; The OrangutanSerial library will put received bytes in to

; the buffer starting at the beginning (receiveBuffer[0]).

; After the buffer has been filled, the library will automatically

; start over at the beginning.

char receive\_buffer[32];

; receive\_buffer\_position: This variable will keep track of which bytes in the

; receive buffer we have already processed. It is the offset(0-31) of the

; next byte in the buffer to process.

unsigned char receive\_buffer\_position = 0;

; send\_buffer: A buffer for sending bytes on USB\_COMM.

char send\_buffer[32];

; sensor\_buffer: A buffer for holding sensor bytes received on USB\_COMM.

;char sensor\_buffer[5];

char mode[2]; ; Changed to single char 3/22/13 -ME

char result[20];

int test = 10;

unsigned int pb\_delay = 500;

int flipper2 = 0; ; allows alternating drumstick beats for two robot arms

int byte\_counter = 0;

; wait\_for\_sending\_to\_finish: Waits for the bytes in the send buffer to

; finish transmitting on USB\_COMM. We must call this before modifying

; send\_buffer or trying to send more bytes, because otherwise we could

; corrupt an existing transmission.

void wait\_for\_sending\_to\_finish()

{

while(!serial\_send\_buffer\_empty(USB\_COMM))

serial\_check(); ; USB\_COMM port is always in SERIAL\_CHECK mode

}

; process\_received\_byte: Responds to a byte that has been received on

; USB\_COMM. If you are writing your own serial program, you can

; replace all the code in this function with your own custom behaviors.

void process\_received\_byte(char byte)

{

;Orangutan LCD user interface initialization

clear(); ; clear LCD

print("Byte Received");

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("RX: ");

delay\_ms(750);

/\*

byte = '3';\*/

switch(byte)

{

; State Machine-style setup for incoming Serial values; expecting ':::'

; then single byte over Serial connection. Increment 'byte\_counter'

; for each ':' until we have three, then next Serial byte is valid.

; Single byte is BPM with granularity of 6 from range 60-120.

case ':':

byte\_counter += 1;

print\_character(byte);

break;

case '0':

test = 0;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '1':

test = 1;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '2':

test = 2;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '3':

test = 3;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '4':

test = 4;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '5':

test = 5;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '6':

test = 6;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '7':

test = 7;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '8':

test = 8;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

case '9':

test = 9;

print\_long(test);

delay\_ms(400);

byte\_counter += 1;

break;

; Default is to place byte in 'send\_buffer' until finished

default:

wait\_for\_sending\_to\_finish();

send\_buffer[0] = byte;; ^ 0x20;

break;

}

}

void check\_for\_new\_bytes\_received()

{

while(serial\_get\_received\_bytes(USB\_COMM) != receive\_buffer\_position)

{

; Process the new byte that has just been received.

process\_received\_byte(receive\_buffer[receive\_buffer\_position]);

; Increment receive\_buffer\_position, but wrap around when it gets to

; the end of the buffer.

if (receive\_buffer\_position == sizeof(receive\_buffer)-1)

{

receive\_buffer\_position = 0;

}

else

{

receive\_buffer\_position++;

}

}

}

int main()

{

servos\_start(demuxPins, sizeof(demuxPins));

; Set the servo speed to 150. This means that the pulse width

; will change by at most 15 microseconds every 20 ms. So it will

; take 1.33 seconds to go from a pulse width of 1000 us to 2000 us.

set\_servo\_speed(0, init\_speed);

set\_servo\_speed(1, init\_speed);

set\_servo\_speed(2, init\_speed);

set\_servo\_speed(3, init\_speed);

; Make all the servos go to a neutral position.

set\_servo\_target(0, rt\_shoulder\_rot); ;right shoulder rotation

set\_servo\_target(1, rt\_elbow); ;right elbow

set\_servo\_target(2, lt\_shoulder\_rot); ;left shoulder rotation

set\_servo\_target(3, lt\_elbow); ;left elbow

;More user information for the interface

clear(); ; clear the LCD

print("Robot Drummer");

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Send BPM Mode");

delay\_ms(3000);

; Set the baud rate in bits per second. Each byte takes ten bit

; times.

serial\_set\_baud\_rate(USB\_COMM, 115200);

; Start receiving bytes in the ring buffer.

serial\_receive\_ring(USB\_COMM, receive\_buffer, sizeof(receive\_buffer));

;Main Loop for performing drum beats

while(1)

{

; USB\_COMM is always in SERIAL\_CHECK mode, so we need to call this

; function often to make sure serial receptions and transmissions

; occur.

serial\_check();

; Deal with any new bytes received unless we have a complete sample

; of three ':' bytes, then 4th byte is desired BPM byte

if (byte\_counter < 4)

{

check\_for\_new\_bytes\_received();

}

;Mode value key for Beats Per Minute (BPM) granularity:

; 0 = 60-65 BPM

; 1 = 66-71 BPM

; 2 = 72-77 BPM

; 3 = 78-83 BPM

; 4 = 84-89 BPM

; 5 = 90-95 BPM

; 6 = 96-101 BPM

; 7 = 102-107 BPM

; 8 = 108-113 BPM

; 9 = 114-120 BPM

; The 'flipper2' variable in this section and the next makes sure that

; the drumming arms alternate beats. Only one of the two drumming arms

; strikes the drum per beat, and the other is up in the air ready to

; strike on the next beat.

if ( flipper2 % 2 != 0 )

{

set\_servo\_speed(0, init\_speed);

set\_servo\_speed(1, init\_speed);

set\_servo\_speed(2, init\_speed);

set\_servo\_speed(3, init\_speed);

; Shoulder servos are static

; Right arm strikes drum

; Left arm raises

set\_servo\_target(0, rt\_shoulder\_rot\_lt); ;right shoulder rotation

set\_servo\_target(1, rt\_elbow\_dn); ;right elbow

set\_servo\_target(2, lt\_shoulder\_rot\_rt); ;left shoulder rotation

set\_servo\_target(3, lt\_elbow\_up); ;left elbow

}

else

{

set\_servo\_speed(0, init\_speed);

set\_servo\_speed(1, init\_speed);

set\_servo\_speed(2, init\_speed);

set\_servo\_speed(3, init\_speed);

; Shoulder servos are static

; Right arm raises

; Left arm strikes drum

set\_servo\_target(0, rt\_shoulder\_rot\_lt); ;right shoulder rotation

set\_servo\_target(1, rt\_elbow\_up); ;right elbow

set\_servo\_target(2, lt\_shoulder\_rot\_rt); ;left shoulder rotation

set\_servo\_target(3, lt\_elbow\_dn); ;left elbow

}

flipper2 += 1; ; increment flipper2 toggle value

;Robot Controller Display and BPM functionality

;This is where the delay occurs for calculated BPM values

if (test == 0) ; 0 = 60-65 BPM

{

clear(); ; clear the LCD

print("BPM = 60-65"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(500);

byte\_counter = 0; ;reset counter

}

else if (test == 1) ; 1 = 66-71 BPM

{

clear(); ; clear the LCD

print("BPM = 66-71"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(440);

byte\_counter = 0; ;reset counter

}

else if (test == 2) ; 2 = 72-77 BPM

{

clear(); ; clear the LCD

print("BPM = 72-77"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(400);

byte\_counter = 0; ;reset counter

}

else if (test == 3) ; 3 = 78-83 BPM

{

clear(); ; clear the LCD

print("BPM = 78-83"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(360);

byte\_counter = 0; ;reset counter

}

else if (test == 4) ; 4 = 84-89 BPM

{

clear(); ; clear the LCD

print("BPM = 84-89"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(345);

byte\_counter = 0; ;reset counter

}

else if (test == 5) ; 5 = 90-95 BPM

{

clear(); ; clear the LCD

print("BPM = 90-95"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(335);

byte\_counter = 0; ;reset counter

}

else if (test == 6) ; 6 = 96-101 BPM

{

clear(); ; clear the LCD

print("BPM = 96-101"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(310);

byte\_counter = 0; ;reset counter

}

else if (test == 7) ; 7 = 102-107 BPM

{

clear(); ; clear the LCD

print("BPM = 102-107"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(290);

byte\_counter = 0; ;reset counter

}

else if (test == 8) ; 8 = 108-113 BPM

{

clear(); ; clear the LCD

print("BPM = 108-113"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(270);

byte\_counter = 0; ;reset counter

}

else if (test == 9) ; 9 = 114-120 BPM

{

clear(); ; clear the LCD

print("BPM = 114-120"); ; display BPM

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Mode: ");

print\_long(test);

green\_led(TOGGLE);

delay\_ms(250);

byte\_counter = 0; ;reset counter

}

else

{

green\_led(TOGGLE);

clear(); ; clear the LCD

print("Robot Drummer"); ; default if no BPM is sent over Serial

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Send BPM Mode");

delay\_ms(pb\_delay);

}

;Button Interface for Orangutan Robot Controller

;Increase or Decrease BPM (or send fun message!)

; If the user presses the middle button, send "Robots Rule!"

; and wait until the user releases the button.

if (button\_is\_pressed(MIDDLE\_BUTTON))

{

wait\_for\_sending\_to\_finish();

memcpy\_P(send\_buffer, PSTR("Robots Rule!\r\n"), 12);

serial\_send(USB\_COMM, send\_buffer, 12);

send\_buffer[12] = 0; ; terminate the string

clear(); ; clear the LCD

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("TX: ");

print\_long(test);

delay\_ms(2000);

byte\_counter = 0; ; reset detect cycle by pressing button

; Wait for the user to release the button. While the processor is

; waiting, the OrangutanSerial library will not be able to receive

; bytes from the USB\_COMM port since this requires calls to the

; serial\_check() function, which could cause serial bytes to be

; lost. It will also not be able to send any bytes, so the bytes

; bytes we just queued for transmission will not be sent until

; after the following blocking function exits once the button is

; released.

wait\_for\_button\_release(MIDDLE\_BUTTON);

}

; If the user presses the TOP button, increment delay by 10 ms

;and display the new Millisecond delay used

if (button\_is\_pressed(TOP\_BUTTON))

{

wait\_for\_sending\_to\_finish();

clear(); ; clear the LCD

print("Delay Up");

if (pb\_delay <= 500)

{

pb\_delay = pb\_delay + 10;

}

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Milliseconds:");

print\_long(pb\_delay);

delay\_ms(250);

byte\_counter = 0; ; reset detect cycle by pressing button

wait\_for\_button\_release(TOP\_BUTTON);

}

; If the user presses the BOTTOM button, decrement delay by 10 ms

;and display the new Millisecond delay used

if (button\_is\_pressed(BOTTOM\_BUTTON))

{

wait\_for\_sending\_to\_finish();

clear(); ; clear the LCD

print("Delay Down");

if (pb\_delay >= 50)

{

pb\_delay = pb\_delay - 10;

}

lcd\_goto\_xy(0, 1); ; go to start of second LCD row

print("Milliseconds:");

print\_long(pb\_delay);

delay\_ms(200);

byte\_counter = 0; ; reset detect cycle by pressing button

wait\_for\_button\_release(BOTTOM\_BUTTON);

}

}

}

1. **Host MATLAB Code**

control.m

function output=control\_accurate(song1, bandlimits, maxfreq)

% CONTROL takes in the names of two .wav files, and outputs their

% combination, beat-matched, and phase aligned.

%

% SIGNAL = CONTROL(SONG1, SONG2, BANDLIMITS, MAXFREQ) takes in

% the names of two .wav files, as strings, and outputs their

% sum. BANDLIMITS and MAXFREQ are used to divide the signal for

% beat-matching

%

% Defaults are:

% BANDLIMITS = [0 200 400 800 1600 3200]

% MAXFREQ = 4096

if nargin < 1, song1 = 'None'; end

if nargin < 2, bandlimits = [0]; end

if nargin < 3, maxfreq = 16384; end

% Length (in power-2 samples) of the song

sample\_size = floor(16\*maxfreq);

scaling = 0.73; % Experimentally derived

% Takes in the two wave files

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

%%%%%% RECORDING LOGIC %%%%%%%%%%%%

if (strcmp(song1, 'None'))

recObj = audiorecorder;

disp('Start of Recording')

recordblocking(recObj, 10);

disp('End of Recording');

x1 = getaudiodata(recObj);

short\_sample = x1;

else

x1 = wavread(song1);

short\_song = x1;

short\_length = length(x1);

start = floor(short\_length/2 - sample\_size/2);

stop = floor(short\_length/2 + sample\_size/2);

% Finds a 5 second representative sample of each song

short\_sample = short\_song(start:stop);

end

% Implements beat detection algorithm for each song

a = filterbank(short\_sample, bandlimits, maxfreq);

b = hwindow(a, 0.1, bandlimits, maxfreq);

c = diffrect(b, length(bandlimits));

% Recursively calls timecomb to decrease computational time

d = timecomb(c, 5, 60, 240, bandlimits, maxfreq);

e = timecomb(c, .5, d-2, d+2, bandlimits, maxfreq);

f = timecomb(c, .1, e-.5, e+.5, bandlimits, maxfreq);

g = timecomb(c, .01, f-.1, f+.1, bandlimits, maxfreq);

h = floor(scaling\*g);

% We want 60-120 BPM, so scale harmonics into range. Assume 240 Max

% and 15 Min BPM in audio input sample.

if ((h > 120) || (h < 60)) % Only scale if out of range

if (h < 30 )

h = 3\*h; %double if less than 60, assume never below 30BPM

elseif ((h > 30) && (h < 60))

h = 2\*h; %double if less than 60, assume never below 30BPM

elseif (h > 121)

h = 0.5\*h; %halve if more than 120 but less than 180

%assume never over 300

end

end

short\_song\_bpm = floor(h);

output = short\_song\_bpm;

filterbank.m

function output = filterbank(sig, bandlimits, maxfreq)

% FILTERBANK divides a time domain signal into individual frequency

% bands.

%

% FREQBANDS = FILTERBANK(SIG, BANDLIMITS, MAXFREQ) takes in a

% time domain signal stored in a column vector, and outputs a

% vector of the signal in the frequency domain, with each

% column representing a different band. BANDLIMITS is a vector

% of one row in which each element represents the frequency

% bounds of a band. The final band is bounded by the last

% element of BANDLIMITS and MAXFREQ.

%

% Defaults are:

% BANDLIMITS = [0 200 400 800 1600 3200]

% MAXFREQ = 4096

%

% This is the first step of the beat detection sequence.

%

% See also HWINDOW, DIFFRECT, and TIMECOMB

if nargin < 2, bandlimits=[0 200 400 800 1600 3200]; end

if nargin < 3, maxfreq=4096; end

dft = fft(sig);

n = length(dft);

nbands = length(bandlimits);

% Bring band scale from Hz to the points in our vectors

for i = 1:nbands-1

bl(i) = floor(bandlimits(i)/maxfreq\*n/2)+1;

br(i) = floor(bandlimits(i+1)/maxfreq\*n/2);

end

bl(nbands) = floor(bandlimits(nbands)/maxfreq\*n/2)+1;

br(nbands) = floor(n/2);

output = zeros(n,nbands);

% Create the frequency bands and put them in the vector output.

for i = 1:nbands

output(bl(i):br(i),i) = dft(bl(i):br(i));

output(n+1-br(i):n+1-bl(i),i) = dft(n+1-br(i):n+1-bl(i));

end

%output(1,1)=0;

hwindow.m

function output = hwindow(sig, winlength, bandlimits, maxfreq)

% HWINDOW rectifies a signal, then convolves it with a half Hanning

% window.

%

% WINDOWED = HWINDOW(SIG, WINLENGTH, BANDLIMITS, MAXFREQ) takes

% in a frequecy domain signal as a vector with each column

% containing a different frequency band. It transforms these

% into the time domain for rectification, and then back to the

% frequency domain for multiplication of the FFT of the half

% Hanning window (Convolution in time domain). The output is a

% vector with each column holding the time domain signal of a

% frequency band. BANDLIMITS is a vector of one row in which

% each element represents the frequency bounds of a band. The

% final band is bounded by the last element of BANDLIMITS and

% MAXFREQ. WINLENGTH contains the length of the Hanning window,

% in time.

%

% Defaults are:

% WINLENGTH = .4 seconds

% BANDLIMITS = [0 200 400 800 1600 3200]

% MAXFREQ = 4096

%

% This is the second step of the beat detection sequence.

%

% See also FILTERBANK, DIFFRECT, and TIMECOMB

if nargin < 2, winlength = .4; end

if nargin < 3, bandlimits = [0 200 400 800 1600 3200]; end

if nargin < 4, maxfreq = 4096; end

n = length(sig);

nbands = length(bandlimits);

hannlen = winlength\*2\*maxfreq;

hann = [zeros(n,1)];

% Create half-Hanning window.

for a = 1:hannlen

hann(a) = (cos(a\*pi/hannlen/2)).^2;

end

% Take IFFT to transfrom to time domain.

for i = 1:nbands

wave(:,i) = real(ifft(sig(:,i)));

end

% Full-wave rectification in the time domain.

% And back to frequency with FFT.

for i = 1:nbands

for j = 1:n

if wave(j,i) < 0

wave(j,i) = -wave(j,i);

end

end

freq(:,i) = fft(wave(:,i));

end

% Convolving with half-Hanning same as multiplying in

% frequency. Multiply half-Hanning FFT by signal FFT. Inverse

% transform to get output in the time domain.

for i = 1:nbands

filtered(:,i) = freq(:,i).\*fft(hann);

output(:,i) = real(ifft(filtered(:,i)));

end

diffrect.m

function output=diffrect(sig,nbands)

% DIFFRECT differentiates signal, then half-wave rectifies the result.

%

% DIFF = DIFFRECT(SIG, NBANDS) takes in a time domain signal

% stored in a vector with each column representing a different

% frequency band. The number of frequency bands is passed in

% through NBANDS.

%

% Defaults are:

% NBANDS = 6

%

% This is the third step of the beat detection sequence

% See also FILTERBANK, HWINDOW, and TIMECOMB

if nargin <2, nbands=6; end

n = length(sig);

output=zeros(n,nbands);

for i = 1:nbands

for j = 5:n

% Find the difference from one sample to the next

d = sig(j,i) - sig(j-1,i);

if d > 0

% Retain only if difference is positive (Half-Wave rectify)

output(j,i)=d;

end

end

end

timecomb.m

function output = timecomb(sig, acc, minbpm, maxbpm, bandlimits, maxfreq)

% TIMECOMB finds the tempo of a musical signal, divided into

% frequency bands.

%

% BPM = TIMECOMB(SIG, ACC, MINBPM, MAXBPM, BANDLIMITS, MAXFREQ)

% takes in a vector containing a signal, with each band stored

% in a different column. BANDLIMITS is a vector of one row in

% which each element represents the frequency bounds of a

% band. The final band is bounded by the last element of

% BANDLIMITS and MAXFREQ. The beat resolution is defined in

% ACC, and the range of beats to test is defined by MINBPM and

% MAXBPM.

%

% Defaults are:

% ACC = 1

% MINBPM = 60

% MAXBPM = 240

% BANDLIMITS = [0 200 400 800 1600 3200]

% MAXFREQ = 4096

%

% Note that timecomb can be recursively called with greater

% accuracy and a smaller range to speed up computation.

%

% This is the last step of the beat detection sequence.

%

% See also FILTERBANK, HWINDOW, and DIFFRECT

if nargin < 2, acc = 1; end

if nargin < 3, minbpm = 60; end

if nargin < 4, maxbpm = 240; end

if nargin < 5, bandlimits = [0 200 400 800 1600 3200]; end

if nargin < 6, maxfreq = 4096; end

n=length(sig);

bpms = [0,0,0,0,0,0,0,0,0,0];

bpms\_cnt = 1;

nbands=length(bandlimits);

% Set the number of pulses in the comb filter

npulses = 3;

% Get signal in frequency domain

for i = 1:nbands

dft(:,i)=fft(sig(:,i));

end

% Initialize max energy to zero

maxe = 0;

for bpm = minbpm:acc:maxbpm

% Initialize energy and filter to zero(s)

e = 0;

fil=zeros(n,1);

% Calculate the difference between peaks in the filter for a

% certain tempo

nstep = floor(120/bpm\*maxfreq);

% Set every nstep samples of the filter to one

for a = 0:npulses-1

fil(a\*nstep+1) = 1;

end

% Get the filter in the frequency domain

dftfil = fft(fil);

% Calculate the energy after convolution

for i = 1:nbands

x = (abs(dftfil.\*dft(:,i))).^2;

e = e + sum(x);

end

% If greater than all previous energies, set current bpm to the

% bpm of the signal

if e > maxe

sbpm = bpm;

bpms(bpms\_cnt) = sbpm;

bpms\_cnt = bpms\_cnt + 1;

maxe = e;

end

end

output = sbpm;